**EQUIPMENTS**

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Description** | **P/N** | **Qty** |
| 1 | [**Inflate/Deflate device**](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-ea-02-00-00a-066a-a.xml) | 303636A | **1** |
| 2 | **Inflate/Deflate device adapters kit (supersedes 304691A)** | 304691B | **1** |
|  | -[Hose](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-ea-03-00-00a-066a-a.xml) | 307426B | 4 |
|  | -[Hose adapter](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-ea-03-00-00a-066a-a.xml) | 307425A | 4 |
|  | -[Float adapter](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-ea-03-00-00a-066a-a.xml) | 314978A | 4 |
| 3 | [**Emergency floats maintenance kit**](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-gf-75-00-00a-066a-a.xml) **:-** | - | **1** |
|  | 1. [Check valves mounting lever](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-gf-75-00-00a-066a-a.xml) | 202313A | 1 |
|  | 1. [Forward float support](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-gf-75-00-00a-066a-a.xml) | 312520A | 1 |
|  | 1. [Inflate-deflate valve key](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-gf-75-00-00a-066a-a.xml) | 202316A | 1 |
|  | 1. [Gluing paddle](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-gf-75-00-00a-066a-a.xml) | 202314A | 1 |
|  | 1. Hoses plug (superseded by 312253B) | 312253A | 1 |
|  | 1. Hoses plug (supersedes 312253A) | 312253B | 1 |
|  | 1. Hoses test tool | 313693A | 1 |
|  | 1. [Left aft float support](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-gf-75-00-00a-066a-a.xml) | 312529A | 1 |
|  | 1. [Right aft float support](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-gf-75-00-00a-066a-a.xml) | 312530A | 1 |
|  | 1. Relief valve test tool | 313692A | 1 |
|  | 1. [Bottle supports installation tool](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-gf-75-00-00a-066a-a.xml) | 315693A | 1 |
| 4 | [**Floats repacking kit**](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-gf-74-00-00a-066a-a.xml) **:-** | 304695A | **1** |
|  | 1. [Passing rope device](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-gf-74-00-00a-066a-a.xml) | 202295A | 1 |
|  | 1. [Closure rope pulling tool](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-gf-74-00-00a-066a-a.xml) | 202294A | 2 |
|  | 1. [Stress riser string tool](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-gf-73-00-00a-066a-a.xml) | 202318A | 1 |
|  | 1. [Sleeker](file:///C:\Program%20Files%20(x86)\AW189%20IETP\document\dmc-89-a-gf-74-00-00a-066a-a.xml) | 202317A | 2 |
|  | 1. Diffuser cap | 303717A | 2 |
|  | 1. Diffuser cap | 303719A | 2 |

**SUPPLIES**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **No.** | **Description** | **Specification** | **Trade name** | **Supplier** | **Qty** |
| 1 | Nylon cord | MIL-C-5040 type III | - | - | 1 roll |
| 2 | Adhesive tape | ASTM D-5486 TYPE IV CLASS 1 | 231 | Polyken | 1 roll |
| 3 | Polyester cord | FL 20002 | - | Aero Sekur | 1 roll |
| 4 | Repair kit | - | P/N 307273A | Aero Sekur | 1 |

**SPARES**

|  |  |  |
| --- | --- | --- |
| **Description** | **P/N** | **Quantity** |
| EYEPIECE SEALING,LH NSCM A3492 | 311088A | 1 |
| EYEPIECE SEALING,RH NSCM A3492 | 311089A | 1 |
| RELIEF/TOPPING PRESSURE VALVE (NSCM A3492) | P-G10025 | 1 |
| INLET CHECK VALVE WITH BANJO FITTING (NSCM A3492) | 311787A | 1 |
| O-RING (NSCM D9182) | AS568-134 | 1 |
| O-RING (NSCM A3492) (PRE MOD. BT189-135) | S-B10104 | 1 |
| O-RING (NSCM A3492) (POST MOD. BT189-135) | 316683A | 1 |
| INFLATE/DEFLATE PROTECTION (NSCM A3492) (POST MOD. BT189-135) | 304694B | 1 |
| INFLATE/DEFLATE PROTECTION (NSCM A3492) (PRE MOD. BT189-135) | 304694A | 1 |