**LEAD-ACID BATTERY ROOM SPECIAL TOOLS / EQUIPMENT**

|  |  |  |  |
| --- | --- | --- | --- |
| **DESIGNATION** | **CHARACTHERISTIC** | **QTY** | **STATUS** |
| Battery Charger and Discharger with battery connector. | Constant Current Charging Range 0 – 25 ADC.Constant Current Load Bank Range 0 – 50 ADC.Constant Voltage Charging Range 13.90 – 14.50 VDC and 28.20 – 29.00 VDC | 2 | AVAILABLE |
| Digital Multimeter  | Capable to measure Voltage and Current | 1 | AVAILABLE |
| Hydrometer | Range 1.110 to 1.300 s.g. units | 1 | AVAILABLE |
| Infrared Thermometer | Range 0 ºC – 100 ºC  | 1 | AVAILABLE |