|  |  |  |  |
| --- | --- | --- | --- |
| **EMERGENCY LIFE RAFT** |  |  |  |
|  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Description** | **P/N** | **S/N** | **D.O.M** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

**COMPONENT DETAIL:** |  |  |  |
| **1.** | **UNFOLDING** |  |  |  |
|  | **Warning:****The life raft surface is easily damaged by sharp or abrasive object. Do not use pointed or sharp edges tools when you touch or move the life raft. Do not put the life raft on surfaces which have sharp edges or abrasive objects. Do not wear clothes that can damage the life raft fabric.****CAUTION:** Only approved persons are permitted to do this procedure. |  |  |  |
|  | Unfold the LH & RH life raft. I.A.W. AW139 AMP 39-A-25-62-07-02A-91LA-K.Remarks: |  |  |  |
| **2** | **DETAILED INSPECTION** |  |  |  |
|  | **CAUTION:*** The life raft surface is easily damaged by sharp or abrasive objects. Be careful not to damage the life raft during this procedure.
* Only approved persons are permitted to do this procedure.
 |  |  |  |
|  | Perform detailed inspectionI.A.W. AW139 AMP 39-A-25-62-07-02A-31AA-K.Remarks: |  |  |  |
| **3** | **LEAK CHECK** |  |  |  |
|  | **CAUTION:*** Only approved persons are permitted to do this procedure.
* You must do this procedure in a clean and dry area. The work area must be of sufficient dimensions. Its surface must be smooth and has sufficient protections to prevent damage to the life raft.
* Be careful not to put unwanted and sharp objects on the fabric parts of the life raft.
* Do not put fluids or other unwanted materials such as solvents or greases on the work area and on the life raft.
 |  |  |  |
|  | Perform leak check of the LH & RH life raft. I.A.W. AW139AMP 39-A-25-62-07-02A-364A-K.Remarks:  |  |  |  |
|  |

|  |  |  |
| --- | --- | --- |
| **Time** | **Temperature** **(°C)** | **Chamber Air Pressure (PSI)** |
| Initial |  |  |
| 30 min |  |  |
| 60 min |  |  |

Remarks: |  |  |  |
|  | **Leak check of pressure relief valve.**Remarks: |  |  |  |
| 3.1.5 | Fill in Appendix 1 for replacement of parts.Remarks: |  |  |  |
| 3.1.6 | Perform FOD inspection.Remarks: |  |  |  |
| **4** | **FOLDING** |  |  |  |
| 4.1 | Fold the life raft.I.A.W AW139 AMP 39-A-25-62-07-02A-91LA-K.Remarks:  |  |  |  |

**APPENDIX 1**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ITEM REF.** | **PART NO.** | **DESCRIPTION** | **SERIAL NO.** | **APPROVED CERT NO.** | **QTY** |
| **ON**  | **OFF** |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

TABLE 1: PART/COMPONENT REPLACEMENT DETAILS