1. Milliohmmeter (Model: RS PRO ILOM-508A)
2. MPFR GROUND REPLAY CABLE (4 SETS)

|  |  |  |  |
| --- | --- | --- | --- |
| NO | DESCRIPTION | P/N | QTY |
| 1 | CONNECTOR | D38999/26WF3SN | 4 EA |
| 2 | BACKSHELL | M85049/38-19W | 4 EA |
| 3 | AUX CONNECTOR | MS3456W10SL-4P | 4 EA |
| 4 | BACKSHELL | M85049/52-1-10W | 4 EA |
| 5 | BOOT SHRINK | 382A072-25-0 | 4 EA |
| 6 | WIRE 22 AWG 2 CONDUCTOR | M27500-22TG2T14 | 200 FT |

1. MAIN LANDING GEAR TEST BOX (4 SETS)

|  |  |  |  |
| --- | --- | --- | --- |
| NO | DESCRIPTION | P/N | QTY |
| 1 | BOX | 1550C | 4 EA |
| 2 | SWITCH | MS24524-23 (STL1-3) | 8 EA |
| 3 | CONNECTOR | D38999/26WB35PN | 8 EA |
| 4 | BACKSHELL | M85049/38-11W | 8 EA |
| 5 | BOOTSHRINK | 382A012-25-0 | 4 EA |
| 6 | WIRE 22AWG 3 CONDUCTOR | M27500-22TG3T14 | 500 FT |

1. GCU TEST BOX (2 SETS)

|  |  |  |  |
| --- | --- | --- | --- |
| NO | DESCRIPTION | P/N | QTY |
| 1 | BOX, METAL ENCLOSURE | 1590PPBK | 2 EA |
| 2 | CONNECTOR | D38999/26WA35PN | 2 EA |
| 3 | BACKSHELL | M85049/38-9W | 2 EA |
| 4 | TOGGLE SWITCH | 1 TL1-7 | 2 EA |

1. EQUIPMENT’S ACCESSORIES

|  |  |  |  |
| --- | --- | --- | --- |
| NO | DESCRIPTION | P/N | QTY |
| 1 | #6 PIDG RING, TERMINAL LUG | 36152 | 60 EA |
| 2 | HEAT SHRINK TUBING | HIX-1/4 | 100 FT |
| 3 | HEAT SHRINK TUBING | HIX-1/2 | 100 FT |